Cross Lake Project (1983-86)

Geologist P.G. Lenton Year 86 STATION 6120
EASTING 560370 NORTHING 6026640 ZONE 14 DATUM NAD83
Date of mapping 06/14/1986

STRUCTURAL DATA

Layering:
Layering type | Strike | Dip | top Direction
inclusion layering | 296 | 38 |

Planar Structures:
Structure type | Strike | Dip | Separation
schistosity | 11 | 69 |
fault | 246 | 79 | sinistral

-cuts and offsets late pegs. 15 cm

PETROLOGIC DATA

Rock Number: 1

Rock Type: multi-component schlieric gneiss
Field Description:

-as previous-late MG-granite adn pegs. sitting?? up old schlieric gneiss largely derived from PORT GRDR
-this material bears some resemblance to WJC but I wouldn't want to correlate them now
-the layering measurement is rough but represents trend of old gneissic layering (schlieren, white TNLT and lit etc.) in old gneiss that is crossed by strong later (post GRNT) fabric that causes intense isoclinal folding in gneiss

Manitoba Geological Survey, 2017