Cross Lake Project (1983-86)

Geologist P.G. Lenton Year 84 STATION 5467
EASTING 573505 NORTHING 6060630 ZONE 14 DATUM NAD83
Date of mapping 06/24/1984

STRUCTURAL DATA

Layering:
Layering type | Strike | Dip | top Direction
bedding | 309 | 79 |

Linear Structures
Type | Plunge | Azimuth
clast elongation | 86 | 23

-deformation consists of extreme rotting and acrenulated fold pattern trending 209 degrees

PETROLOGIC DATA

Rock Number: 1

Rock Type:
Field Description:

-interlayered sequence of 1 to 2 m conglomerate beds and massive to poorly cross bedded feldspathic lithic arenite
-the sandstones average less than 1 m thick
-minor toumaline is diseminated through out
-the major clast type in the conglomerate is sedimentary
-dominantly siltstone and greywacke
-mafic clasts are rare
-granitics vary from 5 to 15 %
-high level mafic porphyrys represent 5%
-the conglomerate appear to be sheets not trough deposits
-it is apparent that has been a major providence change into a source of lithified sediments
-sample B is lineate conglomerate

Manitoba Geological Survey, 2017