Cross Lake Project (1983-86)

Geologist P.G. Lenton Year 84 STATION 5432
EASTING 575485 NORTHING 6060070 ZONE 14 DATUM NAD83
Date of mapping 06/20/1984

STRUCTURAL DATA

Layering:
Layering type | Strike | Dip | top Direction
bedding | 56 | 88 | S

Planar Structures:
Structure type | Strike | Dip | Separation
schistosity | 35 | 90 |
fault | 61 | 87 |

-tops south on both sides of fault
-sudden transition from sillimanite rich pelitic conglomerate sandstone into muscovite bearing cross bed and trough unit
-transition is at a fault

PETROLOGIC DATA

Rock Number: 1

Rock Type: arenite
Field Description:

-appears to be a thin wedge of sillimanite-bearing material faulted up into staurolite grade sediments
-check sample for muscovite vs. sillimanite
-arenite north of fault are more quartz rich

Manitoba Geological Survey, 2017